
**HD Smart Intelligent Dome Camera XM\_iCSee Simple Operating Manual**

****

Dear users, welcome in the use of this product. Before using the product, please read the operation manual carefully and save the operation manual for the future reference.

**I. Main function description**



**II. Downloading of mobile phone APP**

**Scan the following QR code to download the APP（Suitable for Android and IOS）**

****

**III. How to add the camera**




1. **Wired Connection**



① Please connect the network cable to the device cable. The other end of the cable is connected to the router or VCR. The camera is powered on, waits for starting and completes the self-test (if the self-test fails, press the recovery key for a long time to restore the factory settings).

1. **Wireless LAN connection**

Note: This product only supports 2.4GHZ format WIFI. Before adding the device, please make sure that your router is 2.4GHZ WIFI, and the mobile phone is connected to 2.4GHZ WIFI.

1. The camera is powered on, waits for starting and completes the self-test (if the self-test fails, press the recovery key for a long time to restore the factory settings).
2. After the mobile phone is connected to WIFI, click "Add Camera" on the main interface of the APP to select "Add My Device (Recommended)" (the SN QR code above the machine) or "Add Device on the same router".
3. Type in your own default password, click OK, then modify the device name and click Save.

④ The camera shows online and the preview could be conducted by clicking the device name.   

**3. AP hotspot addition**

① When the camera is powered on and the system is started, keep short press of Retest button for three times. A voice prompt "Enter Direct Mode" will appear (if the self-test fails, press the recovery key for a long time to restore the factory settings).


② Open the APP and click Add my device (AP mode), select the WiFi name starting with camera-, and type in the password1234567890. (If you change your password, enter your modified password) as shown in the figure below

③ After the successful connection, the application method is the same as the wireless connection operation.


 

**IV. Function introduction （Sliding screen rotating equipment）**

**① Introduction to the real-time preview interface**



**② Mode switch**

****

**③ Smart alert settings**




1. **Command list of Shortcut Actions of presetting bit (For video recorder)**

**Stakes**：The default manufacturer's network XiongMai RX ball docking super look at the cloud control of mobile phone software is right to dock the cloud control of the computer terminal and the video recorder, right to left is opposite, the "84" command needs to be invoked, the cloud control of the computer terminal and the video recorder can be used normally.

|  |
| --- |
| Function and mode of operation. |
| Camera Universal Address 255. |
| Enabling Cruise Line to Call Preset No. 71. |
| Cruise Reserve Stays for 4 seconds and Calls Reserve 75. |
| Cruise Reset Stays for 8 seconds and Calls Reset 76. |
| Cruise Reserve Stays for 10 seconds and Calls Reserve 77. |
| Cruise Reset Stays 15 seconds and Calls Reset 78. |
| Cruise Reserve Stays for 20 seconds and Calls Reserve 79. |
| Setting the left limit A to call the 91 preset. |
| Setting right limit B to call 92 preset. |
| Enabling A and B two-point scanning to invoke preset number 93. |
| Clear A and B Scan and Call No. 94 Preposition. |
| The scanning speed of point A and B calls the preset position 65, 66, 67 and 68, and the corresponding speed is 5, 10, 20 and 30 degrees per second. |
| Clear all preset bits and call No. 60 preset. |
| Open the Ball Machine Menu and Call Preset No. 95. |
| Yuntai left and right control forward call No. 84 preset. |
| Right and left control of Yuntai invokes No. 85 preset. |
| Restore the factory to call the No. 96 preset. |

**⑤ Setup management **

**Modify camera language, volume, image position, etc.**

****

**Modify the camera to view the password camera time zone**

**Set the recording duration, application time and code stream**

**Modify the camera's time zone and time**

**V. Common problems**

**①. Can't the equipment be added in the cable connection method?**

(1) Please ensure that the device has been restored to the factory settings before adding the device. Keep long press of the reset button until the voice prompt is sent out.

(2) The camera fails to obtain the IP. Please confirm that the number of internet devices mounted on the target router or recorder is within a reasonable range. Otherwise, please reduce the mounted device or restart the router before attempting.   
**②. The configuration of AP connection mode is unsuccessful.**

⑴Wrong wifi password input

(2) Plug and unplug the power supply again to restart the device.

(3) Check whether the direct connection mode is entered.

**③. Why is the TF card plugged, choose continuous video, or intermittent?**

(1) Make sure that the video's view path is selected as the TF card. Format the TF card at first. If the TF card is still intermittent, it may have the dead pixel. 2 If the TF card is lost once or twice a day for about 2 minutes, the camera releases the memory for restarting, which is normal.

**④. Why isn't the TF card recognized ?**

(1) Firstly, confirm whether the TF card meets the requirements. If the network is unstable, the TF card will also not be recognized. You can change the video view to standard definition to avoid failing to load SD card status due to poor network.

**⑤. Why is the TF card used and is the video file blank?**

(1) If the card is used all the time, or if there is video originally which suddenly disappears, firstly, confirm whether the TF card status is normal in the APP, and the recording mode is not "no video". If the status is abnormal, or it is normal but there is no recording, format the card before inserting it for usage. In case of failure, the card's service life expires. Please replace it with a new TF card.

**⑥. Why can't the camera conduct the double light alert?**

(1) Firstly, confirm that the notification push permission of the APP in the mobile phone setting is opened, and then open the "smart alert" in the notification setting of the APP. And the current time is not in the scheduled time period of the stop notification.

**⑦. What should we do if the display camera is disconnected?**

(1) Firstly, confirm whether the power supply and the network are normal, and then power off the camera for restarting in case of no problem. If the connection is still lost after restarting, please remove the camera in the APP and then add it again.

**⑧. Why is there a circle in the middle when you watch the video screen and is the scene stuck?**

(1) The circle indicates that the video is loading. Please check whether the network connected to the camera and mobile phone is smooth.

**⑨. Can the camera be used only in the same LAN?**

(1) No, after the initial connection, the mobile phone can access the device by connecting any wireless network when the network connected to the device keeps unchanged.

**⑩. The camera couldn't operate normally or start?**

⑴ Please make sure the camera is connected to the mobile phone network successfully.

(2) Keep long press of the camera Retest button, the camera will restart and recover the factory settings.

**After-sales Description**

1.The products shall be subject to the entity. The manual is only used for reference.

2.The product is updated real time. If there is any upgrade without prior notice, please inquire the official website.

3.The instruction contains the basic functions of the product, and the users shall conduct the voluntary contrast operation.

4.If there is any problem in the usage of the camera, please contact your supplier or company in time.

5.We have tried to guarantee the completeness and accuracy of the contents in instruction as far as possible, but part of the data may still have the deviation with the actual condition.

In the case of any doubt and dispute, please refer to the company's final explanation.

1. If you do not follow the guidance in the instructions, any loss caused by it will be borne voluntarily.

 **Notes:**

1. Please modify the user password while using this product to avoid being stolen by criminals.
2. Do not install the device in wet and dusty place which is accessible to children.
3. Please use and store the device within the permissible temperature range. Please do not disassemble the device at will.